Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 146 - LIT-18626-12-95
P. 146

    Operation and handling requirements

               Draining the bilge water         Engine compartment
           NOTICE
           z Do  not  run the engines at full throttle
            when bilge water remains in the engine
            compartment. The bilge water can                                1
            splash into the engines, which can result
            in severe damage.
           z Be sure all drain plugs are tightened be-
            fore  operating your boat. Otherwise,
            water may flood the boat and cause it to
            submerge.                           1  Engine compartment drain plug

                                                To drain the bilge water from the hull:
           Draining the bilge water on land     Remove the  hull drain plug at  the stern  to
           This model is equipped with multiple  drain  drain the water. Check the condition of the O-
           plugs.                               ring on the hull drain plug, and then securely
           Bilge water from the various compartments  install the drain plug.
           flows through drain passages and collects in
           the bottom of the hull. The bilge water can be
           drained from the boat by removing the hull
           drain plugs.

           Ski locker

                                                                          1
                                                1  Hull drain plug

                               1

           1  Drain plug

           138

| 141 142 143 144 145 146 147 148 149 150 151 |