Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-95
P. 75

    Instrument operation

           Warning example
                        Warning title                         Message
           Check Engine                         Stop Port Engine.
           Low Oil Pressure                     Consult YAMAHA dealer.
           Over Temperature
           Check Engine                         Stop Starboard Engine.
           Low Oil Pressure                     Consult YAMAHA dealer.
           Over Temperature
           House Battery                        Low Voltage.
                                                Start engine to recharge the battery.
                                                High Voltage.
           Start Battery                        Low Voltage.
                                                Start engine to recharge the battery.
                                                High Voltage.
           Fuel Level                           Low Fuel Level
           Depth                                Low Depth Level
           Port Engine                          Maintenance Due
           Starboard Engine                     Maintenance Due
           Communication Error                  Port Engine.
                                                Starboard Engine.
                                                SPU25-15.
                                                Depth transducer.
                                                Joystick.
                                                Pump controller.
                                                SPU25-15, joystick and depth transducer.
                                                Engine CAN.
                                                Stereo.
                                                GPS.

                                                                                 67

| 70 71 72 73 74 75 76 77 78 79 80 |