Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 164 - LIT-18626-12-95
P. 164

    Operation

           TIP:                                    operator falls off, allowing the boat to
           252S / 252SE / 252SD: You can also push the  continue to  run and cause an  acci-
           “BLOWER” switch  to ventilate the engine  dent.
           compartment.                         AR250 / SX250 / 252S

           252S                                              1
                                                        2

                                                                      3
                                       1

                                                1  Engine shut-off switch
                                                2  Clip
                                                3  Engine shut-off cord (lanyard)
           1  “BLOWER” switch
                                                252SE / 252XE / 252SD
           252SE / 252SD

                                                                       3
                                      1

                                                           1

                                                           2

                                                1  Engine shut-off switch
           1  “BLOWER” switch
                                                2  Clip
           (4) Attach the engine shut-off cord (lanyard)  3  Engine shut-off cord (lanyard)
              to your PFD. Install the clip onto the en-
                                                TIP:
              gine shut-off switch by pushing the clip
                                                The engines will not start when the clip is re-
              groove over the nut beneath the knob.
                                                moved from the engine shut-off switch.
              Be sure the cord is not wrapped around
                                                (5) Put the remote control levers in the neu-
              the steering wheel or tangled in the con-
                                                   tral position. The starter motors will not
              trols.  WARNING! Check  that the en-
                                                   operate unless the remote control levers
              gine shut-off cord (lanyard) is
                                                   are in neutral.
              attached correctly. If the engine shut-
                                                (6) AR250 / SX250 / 252S: Turn  the  main
              off cord (lanyard) is not attached cor-
                                                   switch keys to the start position and re-
              rectly, it may not pull free when the
           156

| 159 160 161 162 163 164 165 166 167 168 169 |