Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-95
P. 52

    Control function operation

           Tilt lever
               WARNING
           z Never touch the tilt lever during opera-
            tion, otherwise the steering wheel could
            suddenly change  position, which may
            lead to an accident.
           z Be sure the steering wheel is locked in
            position after adjustment. If the steering
            wheel is not locked in position, it may
            suddenly change position during opera-
            tion, which may lead to an accident.
           The tilt lever is located  under the steering
           wheel and is used to adjust the tilt of the
           steering wheel. There are 5 positions.

                             1

           1  Tilt lever
           To adjust the tilt:
           (1) Push the lever down, and then move the
              steering wheel up or down to the desired
              position.
           (2) The lever will lock into place when the
              steering wheel is moved into one of the 5
              available positions.
           (3) Make sure that the tilt lever returns to its
              original  position and that  the steering
              wheel is securely locked in place.

           44

| 47 48 49 50 51 52 53 54 55 56 57 |