Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 189 - LIT-18626-12-95
P. 189

    Maintenance

           Periodic maintenance chart
           The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
           Yamaha dealer perform the checks in the following chart. However, maintenance may need
           to be performed more frequently depending on your operating conditions. If you have any
           questions, consult a Yamaha dealer.
           This “√” mark indicates items to be checked and serviced by a Yamaha dealer.
                                                         Initial   Thereafter every
                                                                 50     100   200
                  Item                 Operation                hours   hours   hours
                                                           10
                                                         hours  or 12   or 12   or 24
                                                               months  months  months
                                                                 *1     *1     *1
           Fuel hoses, clamps,   Check for damage, and check con-
           canister, and check   nections and tightening of clamps       √
           valve
                              Check cap for damage, and check
           Fuel filler cap                                               √
                              seal for cracks and deformation
           Fuel tank          Check installation           √             √
           Main switches and
           engine shut-off    Check operation              √             √
           switch
                              Check state of charge and termi-
           Batteries          nals, and check for broken battery         √
                              straps
           Battery leads      Check terminals                            √
           Battery switches   Check operation              √             √
           Multi-function display
           (after completing the   Check lighting          √             √
           pre-operation
           checks)
           Neutral switches
           (AR250 / SX250 /   Check operation              √             √
           252S)
           Hatch interlock
           switches (wet stor-  Check operation            √             √
           age compartment)
           Blowers            Check operation              √             √
           Horn               Check operation              √             √
           Navigation lights  Check lighting               √             √
                              Clean filter, check hoses for dam-
           Electric bilge pump  age, and check tightening of             √
                              clamps
           Other electrical com-  Check operation of shower, stereo,   √  √
           ponents            and other components

                                                                                181

| 184 185 186 187 188 189 190 191 192 193 194 |