Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-95
P. 46

    Control function operation

           such as the circuits for lighting, bilge pump,
           blowers and audio system.                     1           2
                         2
                  1

                                                1  ON position (green)
                                                2  OFF position (red)
           1  Start battery
           2  House battery                     In normal operation, keep the “START” and
                                                “HOUSE” switches in the ON position. Keep
           The battery switch assembly is located in the  the “EMERG PARALLEL” switch in the OFF
           rear underseat storage compartment (port).  position. This setting allows both batteries to
           There are three switches  on  the  battery  be charged automatically while the engines
           switch assembly: the  “START”  switch,  are running.  NOTICE: Do  not turn the
           “HOUSE” switch, and “EMERG PARALLEL”  “HOUSE” switch to the OFF position if the
           switch.                              boat is moored in the water as it will pre-
                                                vent the anchor light from functioning.
                                                If  the start  battery is discharged, turn  the
                          2                 3   “EMERG PARALLEL” switch to the ON posi-
                                                tion to start the engines. Once the engines
                                                are started  or the start battery is charged,
                 1                          4   turn the “EMERG PARALLEL” switch to the
                                                OFF position.

           1  Battery switch assembly
           2  “HOUSE” switch (red)
           3  “EMERG PARALLEL” switch (yellow)
           4  “START” switch (red)

           38

| 41 42 43 44 45 46 47 48 49 50 51 |