Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 129 - LIT-18626-12-95
P. 129

    Equipment operation

                    USB chargers                        Wakeboard tower
           There are the USB chargers on the deck. The  (except for SX250)
           USB charger can be used to charge external  The wakeboard tower is provided as an ele-
           devices.                             vated tow point suitable for wakeboards and
                                                similar towable recreational equipment. The
                                                tow pylon can be used to attach a standard
                                                ski rope or other tow-rope.

                                  1

                                 5V

           1  USB charger

                                                    WARNING
                                                Severe injury or death can result if you ig-
                                                nore any of the following:
                                                z Maximum towing capacity:
             1                                    1 Person, 158 kg (350 lb) max.
                                                z Make sure the tow-rope is securely fas-
                                                  tened to the  tow  pylon on the wake-
           1  USB charger                         board tower.
                                                z Do  not  tow a tube or other inflatable
                                                  from the wakeboard tower. Use the ski
                                                  tow hook on the transom.
                                                z Stay clear of the tow-rope while pulling
                                                  a wakeboard rider or skier.
                                                z Do not climb, hang, or sit on the wake-
                                                  board tower.
                                                z Make sure all knobs or pins securing the
                                                  wakeboard tower are tightened before
                                                  operation and check periodically during
                                                  use.

                                                                                121

| 124 125 126 127 128 129 130 131 132 133 134 |