Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 108 - LIT-18626-12-95
P. 108

    Equipment operation

           (3) Swivel the seat to the desired position. If  To use the armrests:
              it is too easy or too difficult to rotate the  Lower the armrests until they stop.
              seat, adjust the swivel friction by turning
              the swivel friction knob in or out.

                                                                            1

                                   1            1  Armrest

           1  Swivel friction knob              To adjust the backrest angle:
                                                While lifting the adjusting lever on the star-
           (4) Push the lever to its original position.  board side of the seat, move the backrest to
           To flip up the seat bolster:         the desired position.
           Lift up the seat bolster at the front of the seat
           so that it is resting against the backrest.

                                                                                 1
               1                                1  Adjusting lever

           1  Seat bolster                      TIP:
                                                Depending on the direction and position of
                                                the seat, it may not be possible to adjust the
                                                backrest angle.

           100

| 103 104 105 106 107 108 109 110 111 112 113 |