Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-12-95
P. 54

    Instrument operation

           Switch panel                            Multi-function display unit
           In addition to touching the multi-function dis-  operation
           play directly, you can use the switches to op-
                                                Because the multi-function display unit is
           erate various functions.
                                                equipped with a touch screen, you can touch
                       1      2                 the display directly to operate the display
                                                functions.
                                                In addition to touching the display, you can
                                                use the joystick to operate the display func-
                       HORN
                              BILGE
                                                tions.
                                                Touching the multi-function display

           1  “HORN” switch                                NW   N    NE
                                                    FUEL                   DEPTH
           2  “BILGE” switch                        50  %    FLOAT MODE    0  Ft
                                                                   °F
           “HORN” switch                                      Water Temp
           Activates the horn. The horn can be used to  START  V         HOUSE  V
                                                                         11.8
                                                     36.3
           signal other boats as required by the “Rules  Bilge  Blower  Nav  Anchor
           of the road”. (See page 20.)
           The switch light comes on while the horn is
           operating.
                                                Using the joystick
           “BILGE” switch                       This joystick has the following two operation
           Turns the bilge pump on or off. (See page  modes.
           139.)                                z Volume control mode
           The switch light comes on while the bilge  z Navigation control mode
           pump is operating.                   Push the  “VOLUME–(SCROLL)” button to
           TIP:                                 switch the operation mode.
           Even if the bilge pump is turned off, the pump
                                                                 1
           will operate every 2 minutes when the house
           battery switch is in the on position.
                                                                 VOLUME
                                                                 (SCROLL)
                                                             HOME   CANCEL

                                                               CRUISE  CRUISE
                                                               NO WAKE  NO WAKE

                                                1  “VOLUME–(SCROLL)” button

           46

| 49 50 51 52 53 54 55 56 57 58 59 |