Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 122 - LIT-18626-12-95
P. 122

    Equipment operation

                     Anchor light                     Anchor light (SX250)
           (252S / 252SE / 252XE / 252SD)       The boat is equipped with a removable an-
           The anchor light is located at the top center of  chor light. It is also the “all-around” light for
           the wakeboard tower. It is also the “all-  navigation at night or in low-visibility condi-
           around” light for navigation at night or in low-  tions. (See page 63 for information on the an-
           visibility conditions. (See page 89 for informa-  chor light on.)
           tion on the anchor light on.)        The anchor light is stored in the ski locker.
           To use the anchor light:             To set up the anchor light:
           Pull the lock tab, raise the anchor light, and  (1) Open the ski locker. (See page 104.)
           then move the lock tab to its original position
           to lock the anchor light in place.

                                                                            1

                                   1

                                                1  Ski locker

                                                (2) Remove the anchor light from the anchor
           1  Lock tab
                                                   light holder.

                           1

                                                          1
                                                                         2

           1  Anchor light                      1  Anchor light holder
                                                2  Anchor light
           To store the anchor light:
           Pull the lock tab, lower the anchor light, and
           then move the lock tab to its original position
           to lock the anchor light in place.

           114

| 117 118 119 120 121 122 123 124 125 126 127 |