Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 115 - LIT-18626-12-95
P. 115

    Equipment operation

                                                Driver’s side console compartment
                                                The driver’s side console compartment is lo-
                                                cated in front of the helm.
                                                The driver’s side console compartment door
                                                can be used as a partition in the front walk-
                                                through.
                                                To open the driver’s side console compart-
                                                ment, unhook the driver’s side console com-
                               1                partment door latch.

           1  Enclosed head compartment
           There is the head compartment light in the
           enclosed head compartment. To turn on the                      1
           light, turn the head compartment light switch
           to on position. To turn off the light, turn the
           light switch to off position. NOTICE: Be sure                  2
           the head compartment light is turned off
           when no one is in the enclosed head com-
           partment. Leaving the light on can  drain  1  Driver’s side console compartment door
           the battery.                         2  Driver’s side console compartment door latch

                                   1

                                   2
                                                                          1

           1  Head compartment light switch
           2  Head compartment light            1  Driver’s side console compartment
           To close the enclosed head compartment:  To close the driver’s side console compart-
           (1) Close  the enclosed head compartment  ment, close the  driver’s side console com-
              door.                             partment  door, and then hook the latch to
           (2) Turn the lock  handle counterclockwise  securely lock it in place.
              and make sure that the door is securely
              closed.
           (3) Push the lock handle in.

                                                                                107

| 110 111 112 113 114 115 116 117 118 119 120 |