Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 193 - LIT-18626-12-95
P. 193

    Specifications

                           Item                             Specification
           Performance
           Maximum fuel consumption (for each engine)  3-star models
                                                49.7 L/h (13.1 US gal/h, 10.9 Imp.gal/h)
                                                4-star models
                                                43.8 L/h (11.6 US gal/h, 9.6 Imp.gal/h)
           Cruising range at full throttle      3-star models
                                                2.86 hour
                                                4-star models
                                                3.24 hour
           Trolling speed                       1300 ±100 r/min
           Engine
           Number of engines                    2
           Engine type                          Liquid cooled 4-stroke, DOHC
           Number of cylinders                  4
           Engine displacement                  1812 cm 3
           Bore × stroke                        86.0 × 78.0 mm (3.39 × 3.07 in)
           Compression ratio                    11.0 : 1
           Valve clearance-intake (cold)        0.14–0.23 mm (0.0055–0.0091 in)
           Valve clearance-exhaust (cold)       0.28–0.37 mm (0.0110–0.0146 in)
           Lubrication system                   Wet sump
           Cooling system                       Water
           Starting system                      Electric
           Ignition system                      T.C.I.
           Spark plug (NGK)                     LFR6A
           Spark plug gap                       0.8–0.9 mm (0.031–0.035 in)
           Battery capacity                     12 V, 85 Ah
           Charging system                      Flywheel magneto

                                                                                185

| 188 189 190 191 192 193 194 195 196 197 198 |