Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 135 - LIT-18626-12-95
P. 135

    Equipment operation

           (5) Remove the front support poles from the
              wakeboard tower, and  then place  the         1
              poles in the flap of the bimini top.

                                  1

                                                    2

                                                1  Bimini top
                                                2  Lock pin

                                                Installing the bimini top
           1  Front support pole
                                                To install the bimini top:
           (6) Pull the front of the bimini top toward the  When installing the bimini top, simply reverse
              stern, wrap the bimini  top around the  the removal steps, and then make sure that
              main pole, and then install the storage  the lock pins are securely installed.
              cover.

           Trailering with the bimini top
           The bimini top must be secured to the boat
           when it is being trailered. When the boat is
           trailered with a genuine Yamaha boat cover,
           simply store the bimini top in the fully col-
           lapsed position and install the storage cover.
           If a boat cover is not used, wrap an elastic
           cord around the top and secure the ends to
           the tow pylon on the wakeboard tower to re-
           strict movement.

           Removing the bimini top
           To remove the bimini top:
           (1) Store the bimini top. See “Storing the bi-
              mini top”.
           (2) While  supporting the bimini top,  rotate
              the lock pins securing the main pole to
              the wakeboard tower, and then remove
              the top.

                                                                                127

| 130 131 132 133 134 135 136 137 138 139 140 |