Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 171 - LIT-18626-12-95
P. 171

    Operation

           Wind or current pushing boat away from   Pull the throttle/shift paddle (right) to move
           dock:                                the boat forward or pull the throttle/shift pad-
           Slowly approach the dock at about a 45° an-  dle (left) to move the boat in reverse at a slow
           gle. Secure the bow to the dock, and then  speed and dock the boat.
           use engine  thrust  or a boat hook to  gently
           move the stern to the dock.
                                                                      1

                         Wind or current
                                                       2

                                                1  Throttle/shift paddle (right)
                                                2  Throttle/shift paddle (left)
           Wind or current pushing boat toward
           dock:
           Slowly maneuver to a shallow angle and al-
           low the boat to move toward the dock.

                    Wind or current

           No wind or current:
           Approach the dock at a shallow angle. Se-
           cure the bow to the dock, and then use en-
           gine thrust or a boat hook to gently move the
           stern to the dock.
           To dock using the DRiVE mode (252SD):
           Move the remote control levers to the neutral
           position, and then activate the DRiVE mode.
           (See page 79.)

                                                                                163

| 166 167 168 169 170 171 172 173 174 175 176 |