Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 25 - LIT-18626-12-95
P. 25

    Safety information

                Additional equipment                   Hazard information
                  recommendations               Never start the engines or let them run for any
           The following equipment can help make your  length of time in an enclosed area. Exhaust
           boating experience safer and more enjoy-  fumes contain carbon monoxide, a colorless,
           able:                                odorless gas that may cause loss of con-
           z Mooring fenders and lines.         sciousness and death within a short time. Al-
           z Anchor with suitable line (a “Danforth” type  ways operate the boat in an open area.
            anchor and line that is at least 6 times the  It is also important to have the engines off
            depth of the water where you will drop an-  when anyone is using the ladder on models
            chor are recommended).              equipped with  one because of the carbon
           z Manual-type bilge pump.            monoxide in the exhaust gases coming from
           z First-aid kit.                     underneath the step.
           z Waterproof flashlight with extra batteries.
           z Tool kit with assorted screwdrivers, pliers,
            wrenches (including metric  sizes), and
            electrical tape.
           z Oar  or paddle  (look  for one with a  boat
            hook on the other end).
           z Spare parts, such as fuses.
           z Navigation charts for the waters where you
            will be boating.
           z Tow-rope.

                                                                                 17

| 20 21 22 23 24 25 26 27 28 29 30 |