Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 56 - LIT-18626-12-95
P. 56

    Instrument operation

                  Operation buttons             Operating the boat at a steady speed
           In addition to touching the multi-function dis-  (cruise assist)
           play directly, you can use the operation but-  The cruise assist feature is for steady engine
           tons and the controller to operate  various  speed operation when the boat is traveling
           functions.                           above no-wake speeds. The cruise assist is
                                                available for use whenever the engines are
           Controller                           running above 3000 rpm and  below  7000
                                                rpm.
                        1   2 3                 To activate the cruise assist:
                                                (1) Push the remote control levers forward
                           VOLUME
                           (SCROLL)                to open the throttle until the desired en-
                        HOME   CANCEL
                                                   gine speed is reached and both engines
                                                   are operating at the same engine speed.
                                                (2) Push the “CRUISE/NO WAKE” (+) button
                                                   or “CRUISE/NO WAKE” (–) button. When
                         CRUISE  CRUISE
                         NO WAKE  NO WAKE
                                                   the cruise  assist is activated, “Cruise”
                          4   5                    and the cruise assist setting level will be
                                                   displayed under the boat speed.
                   Name          Function
            1  “HOME” button  Displays the home           SE     S      SW
                            screen. (See page 80.)
            2  “VOLUME  –   Switches the joystick
               (SCROLL)” but-  between the volume
               ton          control mode and the
                            navigation control
                            mode. When the main
                            switches are turned to              MPH
                            the on position, the               Cruise +4
                            volume control mode
                            is selected by default.
                                                                   1
            3  “CANCEL” but-  Deselects the current-
               ton          ly selected item.
                                                1  Cruise assist setting level
            4  “CRUISE/NO   Activate and set the
               WAKE” (–) but-  cruise assist, no-wake
               ton          mode, and reverse   z Once the cruise assist is activated, the set
            5  “CRUISE/NO   RPM control. (See the   engine speed can be increased by pushing
               WAKE” (+) but-  following sections.)  the “CRUISE/NO WAKE” (+) button or de-
               ton                                creased by  pushing the  “CRUISE/NO
                                                  WAKE” (–)  button. However, the  adjust-
                                                  ment is limited to a maximum of 8 incre-
                                                  ments above or below the initial cruise
                                                  assist setting. Each time a button is
                                                  pushed, the engine speed will increase or
                                                  decrease approximately 100–200 rpm.

           48

| 51 52 53 54 55 56 57 58 59 60 61 |