Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 107 - LIT-18626-12-95
P. 107

    Equipment operation

                                                (2) Rotate the lever to port (left).

                                         5

                         2   3
                                4
                        1

           1  Rear starboard seat
           2  Starboard engine hood seat        (3) Move  the seat to  the desired  position,
           3  Port engine hood seat                and then release the lever.
           4  Rear port seat
                                                (4) Push the lever to its original position.
           5  Handgrip
                                                To swivel the seat:
                                                (1) Extend the slide/swivel lock lever.
           Driver’s seat
                                                (2) Rotate the lever to starboard (right).
           The driver’s seat can slide forward and rear-
           ward, and the seat can swivel, and the back-
           rest angle can be adjusted. In addition, the
           seat bolster at the front of the seat can be
           flipped up to change the seat style for a
           raised seating position.
           Make sure that the seat is securely locked in
           place before getting underway.
           To slide the seat:
           (1) Extend the slide/swivel lock lever.

                  1
           1  Slide/swivel lock lever

                                                                                 99

| 102 103 104 105 106 107 108 109 110 111 112 |