Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 140 - LIT-18626-12-95
P. 140

    Equipment operation

           (5) Pull the bimini top toward the stern, and  (3) Install  the protective cushions around
              then fold it.                        the poles, and then lower the bimini top
                                                   onto the rear deck.
                                            1

                                                                   2

                                                         1

           1  Bimini top
                                                1  Protective cushion
           (6) Install the storage cover.       2  Bimini top

           Storing the bimini top in the fully   Trailering with the bimini top
           collapsed position                   The bimini top must be secured to the boat
           To store the bimini top in the fully collapsed  when it is being trailered. When the boat is
           position:                            trailered with a genuine Yamaha boat cover,
           (1) Follow the above steps for “Storing the  simply store the bimini top in the fully col-
              bimini top in the upright position”.  lapsed position and install the storage cover.
           (2) While supporting the bimini top, remove  If a boat cover is not used, wrap an elastic
              the lock pins securing the rear support  cord around the top and secure the ends to
              poles to the rear support pole mounting  the ski tow hook to restrict movement.
              brackets, and then secure each rear sup-
              port pole to the main pole using the lock
              pin.

                                    1

           1  Rear support pole

           132

| 135 136 137 138 139 140 141 142 143 144 145 |