Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 126 - LIT-18626-12-95
P. 126

    Equipment operation

                                                To use the shower:
                                                (1) Tap  the “Shower” button to select  the
                                      1            “Shower” button on the system control
                                                   screen to turn the shower pump on.

           1  Filler fitting cap
                                                     Shower  Tower  Courtesy  Dock
           (3) Connect a standard garden hose to the
              filler fitting.                           1
           (4) The  tank is completely full when  water
                                                1  “Shower” button
              flows out from the overflow vent on the
              starboard side of the boat.       (2) Open the swim platform shower cover.
             Shower tank capacity:
               37.8 L (10.0 US gal, 8.3 Imp.gal)

                                                                                1

                                  1

                                                1  Swim platform shower cover
                                                (3) Lift the swim  platform shower  handle
           1  Overflow vent                        and push the flow control button to dis-
                                                   charge water.
           (5) Disconnect the garden hose from the fill-
              er fitting.
           (6) Install the filler fitting cap securely.
           (7) Close the rear platform hatch.

           118

| 121 122 123 124 125 126 127 128 129 130 131 |