Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 114 - LIT-18626-12-95
P. 114

    Equipment operation

           To close the rear underseat storage compart-  To close the rear underseat storage compart-
           ment (starboard), lower the rear starboard  ment (port), lower the rear starboard seat.
           seat.
                                                Enclosed head compartment
           Rear underseat storage compartment   The port console has a large compartment
           (port)                               suitable for use  as an  on-board  changing
           NOTICE                               room and can also accommodate a portable
                                                toilet (not  included).  WARNING! Carbon
           252XE: This storage compartment con-  monoxide (CO) can cause brain damage
           tains a ballast tank. Be careful not to store  or death. Carbon monoxide can be pres-
           items in this area that could be crushed or  ent in this compartment. Signs of carbon
           might damage the ballast tank.       monoxide  poisoning include nausea,
                                                headache,  dizziness, drowsiness, and
           The rear underseat storage compartment
                                                lack of consciousness. Get fresh air if any-
           (port) is located under the rear port seat.
                                                one shows signs of carbon monoxide poi-
           To open the rear underseat storage compart-
                                                soning.
           ment (port), lift the rear port seat up.
                                                To open the enclosed head compartment:
                                                (1) Pull the lock handle out.
                                                (2) Turn the lock handle clockwise, and then
             1                                     open the enclosed head  compartment
                                                   door.

                                                         1
           1  Rear port seat

                                                                              2

                                                1  Lock handle
                                  1             2  Enclosed head compartment door

           1  Rear underseat storage compartment (port)

           106

| 109 110 111 112 113 114 115 116 117 118 119 |