Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 160 - LIT-18626-12-95
P. 160

    Pre-operation checks

           252S

                            1

           1  “HORN” switch
                                                Post-launch checks
                                                Perform the post-launch checks in the pre-
           252SE / 252SD
                                                operation checklist while  the boat  is in  the
                                                water and the engines are running.
                            1
                                                Engine shut-off switch check
                                                Check the engine shut-off switch for proper
                                                operation.
                                                (1) Start the engines. (See page 154 for in-
                                                   formation on starting the engines.)
                                                (2) Pull the engine shut-off cord (lanyard) to
                                                   remove the clip from the engine shut-off
                                                   switch to make sure that the engines
           1  “HORN” switch
                                                   stop immediately.
           Engine shut-off cord (lanyard) check  (3) Make  sure that  the engines cannot  be
           Make sure that the engine shut-off cord (lan-  started with the clip removed from the
           yard) is not damaged. If the cord is damaged,  engine shut-off switch.
           replace it.  WARNING! Never try to repair  AR250 / SX250 / 252S
           the engine shut-off cord (lanyard) or tie it
           together. The engine  shut-off cord (lan-
           yard) may not pull free when the operator
           falls off, allowing the boat to continue to                   1
           run and cause an accident.
                                                                  2

                                                1  Engine shut-off switch
                                                2  Clip

           152

| 155 156 157 158 159 160 161 162 163 164 165 |