Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 112 - LIT-18626-12-95
P. 112

    Equipment operation

           To close the anchor storage compartment:  Ski locker
           Close the  anchor  storage compartment lid,  NOTICE
           and then push it to securely lock it in place.
                                                252XE: This storage compartment con-
           Front underseat storage              tains a  ballast  bag. Do not store sharp
           compartments                         items in this storage compartment to pre-
           The front underseat storage compartment  vent the ballast bag from puncturing.
           (starboard) and front underseat storage com-
                                                The ski locker is located under the floor.
           partment (port) are located  under  the front
                                                To open the ski locker:
           starboard seat and front port seat respective-
                                                (1) Pull the lock handle up.
           ly.
                                                (2) Turn the lock handle clockwise, and then
           To open a front underseat storage compart-
                                                   open the ski locker lid.
           ment, lift the front seat (rear) up.
                                                  1

                                                                                 2
                                   1

                                                1  Lock handle
           1  Front starboard seat (rear)
                                                2  Ski locker lid

                                                                            1
               1

           1  Front underseat storage compartment
                                                1  Ski locker
           To close a front underseat storage compart-  To close the ski locker:
           ment, lower the front seat (rear).   (1) Close the ski locker lid.

           104

| 107 108 109 110 111 112 113 114 115 116 117 |