Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 103 - LIT-18626-12-95
P. 103

    Instrument operation

           Warning example
                       Warning title                        Message
           Check Engine
                                             Stop Port Engine.
           Low Oil Pressure
                                             Consult YAMAHA dealer.
           Over Temperature
           Check Engine
                                             Stop Starboard Engine.
           Low Oil Pressure
                                             Consult YAMAHA dealer.
           Over Temperature
                                             Stop the BCU.
                                             Consult YAMAHA dealer.
                                             Stop Steering.
                                             Consult YAMAHA dealer.
           Check Engine                      Stop Steering.
                                             Open service valve of pump. Move cylinder to center
                                             position. Using the two remote control levers, per-
                                             form the boat steering operation by the engine
                                             speed difference.
                                             Consult YAMAHA dealer.
                                             Low Voltage.
           House Battery                     Start engine to recharge the battery.
                                             High Voltage.
                                             Low Voltage.
           Start Battery                     Start engine to recharge the battery.
                                             High Voltage.
           Fuel                              Low Fuel Level.
           Depth                             Low Depth Level.
                                             Port Engine.
                                             Check Engine CAN.
                                             Starboard Engine.
                                             Check Engine CAN.
                                             SPU25-15.
                                             Check Auxiliary CAN.
                                             Depth Transducer.
                                             Check Auxiliary CAN.
                                             Joystick.
                                             Check Auxiliary CAN.
           Communication Error
                                             SPU25-15, Joystick, Stereo and Depth Transducer.
                                             Check Auxiliary CAN.
                                             BCU.
                                             Check Engine CAN.
                                             No communication with the port engine, the star-
                                             board engine and the BCU.
                                             Stereo.
                                             Check Auxiliary CAN.
                                             GPS.
                                             Check NMEA0183 connection.

                                                                                 95

| 98 99 100 101 102 103 104 105 106 107 108 |