Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 182 - LIT-18626-12-95
P. 182

    Care and storage

           (7) Spray the exterior of  the engines with
              Yamalube Silicone Protectant  &  Lubri-
              cant, or an equivalent. For areas requir-
              ing heavy protection, use Yamashield™.
           (8) Wax the hull  with Yamaclean  Spray
                  ®
              Wax  or other non-abrasive wax de-
              signed  for marine gelcoat.  WARNING!
              Slippery surfaces can cause falls and
              injury. Be careful not  to  apply too
              much wax on deck and gunwale step-
              ping surfaces.  This will  make them
              slippery.
           (9) Wipe  all vinyl and  rubber components,
              such as the seats and engine compart-
              ment seals, with Yamaclean Vinyl Dress-
              ing™ or other quality vinyl protectant.
              NOTICE: Some well-known “protec-
              tant” products on the market can ac-
              tually damage vinyl over time. Consult
              a Yamaha Boat Dealer if you want to
              use a product other than Yamaclean
              Vinyl Protectant.
           (10) Vacuum and hose-off the carpeting as
              necessary.  If needed, use  Yamaclean
                          ®
              Carpet Cleaner  or other quality brand-
              name carpet cleaner  product to clean
              soiled areas. NOTICE: Always dry the
              carpet face up. Never roll up the car-
              pet. Never fold the carpet.
           (11) Wash the fabric of the bimini top with a
              mild natural soap in lukewarm water,
              then rinse. Do not use detergents. Allow
              to air dry thoroughly before storage.

           174

| 177 178 179 180 181 182 183 184 185 186 187 |