Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 106 - LIT-18626-12-95
P. 106

    Equipment operation

                         Seats                    ator or striking a passenger,  which
                                                  could result in an accident.
               WARNING
           Passengers must always sit in a designat-                           1
           ed  seating area, place feet on  the  deck,
           and hold on to the handgrips, handrails, or
           straps when the boat is in motion.
           This  boat  is equipped with the following
           seats.
            1 2 3                    4  5  1

                                                1  Bow filler cushion
                                                These cushions can also be used to create a
                                                temporary center seat.

           1  Handrail
           2  Front port seat (rear)
           3  Front port seat (front)
           4  Front starboard seat (front)                                    1
           5  Front starboard seat (rear)

           Two bow filler cushions are provided for use
           while the boat is not being operated.
                                                1  Bow filler cushion
           These cushions can be used to make a large
           flat area in the bow for use as a sundeck.
           To remove or install the bow filler cushions,
           lift up the front seats (rear).
               WARNING
           z Do not use the bow filler cushions while
            the boat is underway.  A passenger
            could lose balance and fall on the deck
            or overboard, causing injury or death.
           z Stow the cushions securely before oper-
            ating the boat. A loose cushion could be
            blown by the wind, distracting the oper-

           98

| 101 102 103 104 105 106 107 108 109 110 111 |