Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 101 - LIT-18626-12-95
P. 101

    Instrument operation

                       Diagnostics Menu

                       Flush-Out Ballasts
                  Port    Center    Stbd
                  30       30       30
                  OFF      OFF      OFF

              Back

           TIP:
           z The flush-out time cannot be adjusted. The
            default setting is 30 seconds to avoid dam-
            aging a ballast pump when there is no wa-
            ter remaining in a tank and/or to prevent
            excessive battery drain.
           z If the flush-out time is not sufficient to re-
            move all the water from a tank, continue
            the draining process until it is empty. Stop
            the process immediately once all the water
            has been removed from each tank.
            If you have  any questions, consult a
            Yamaha Boat Dealer.

           (5) When finished, tap “x” to return to the
              previous screen.

                                                                                 93

| 96 97 98 99 100 101 102 103 104 105 106 |