Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-95
P. 47

    Control function operation

           Main switches                        Main switch (252SE / 252XE / 252SD)
           (AR250 / SX250 / 252S)               The main switch controls the ignition circuit
           There is a main switch for each engine.  as follows:
           The main  switch controls  the ignition  and
           electrical circuits as follows:                      ON
                                                        OFF
                  OFF      START
                       ON

                                                                           1
                        HORN
                               BILGE

                     1            2
                                                1  Main switch

           1  Main switch (port engine)         OFF:
           2  Main switch (starboard engine)    Ignition circuit is  switched off.  The engines
                                                cannot be started. (The main switch key can
           OFF:                                 be removed.)
           Ignition circuit is switched off.  The engine  ON:
           cannot be started, but other switches will op-  Ignition  circuit is  switched on. (The main
           erate. (The main switch key can be removed.)  switch key cannot be removed.)
           ON:
           Ignition circuit is switched on. (The main  “START/STOP” buttons
           switch key cannot be removed.)       (252SE / 252XE / 252SD)
           START:                               The engines can  be  started or stopped by
           The starter motor will turn to start the engine.  pushing the “START/STOP” buttons. It is
           (When the main switch key is released, it re-  possible to start or stop the engines individu-
           turns automatically to “ON”.)        ally.
           TIP:                                 z PORT: Port engine
           z The engine will not start when the clip is re-  z STBD: Starboard engine
            moved from the engine shut-off switch.
            The starter motor will turn over without the
            cord attached.
           z The main switch will not operate (the starter
            motor  will not turn over) if the “START”
            switch in the rear underseat storage com-
            partment (port) is turned to the OFF posi-
            tion. (See page 37 for more information.)

                                                                                 39

| 42 43 44 45 46 47 48 49 50 51 52 |