Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 77 - LIT-18626-12-95
P. 77

    Instrument operation

           NOTICE                               fuel tank as soon as possible. (See page 134
                                                for information on filling the fuel tank.)
           If the  cause of overheating  cannot be
           found and corrected, take special precau-  Depth warning
           tions to avoid major engine damage while  If the boat enters an area that is shallower
           you return to shore.                 than the water depth set for the depth alarm,
           Single engine overheating — Shut off the  the depth warning will be activated and the
           overheating engine and use the properly  buzzer will sound.
           running engine to return to shore. Operate  If the warning is activated, move the boat to
           at no-wake speed (8 km/h, 5 mph) to pre-  an area that is deeper than the water depth
           vent water from flooding the non-operat-  set for the depth alarm. (See page 64 for in-
           ing engine through the water intake. See  formation on setting the depth alarm.)
           page 49 for  information on the no-wake
           mode.
           Both  engines overheating  — If getting a
           tow from another vessel is not possible,
           operate both engines just slightly above
           idle while you return to shore. If you can be
           towed, refer to “Towing the boat” on page
           198.

           House/Start Battery voltage warning
           If “House Battery” “Start Battery” appears on
           the multi-function display and the buzzer will
           sound, check the battery connections. If the
           battery connections are clean and tight and
           the  warning indication continues, have a
           Yamaha Boat Dealer check the charging sys-
           tem.

           Communication error warning
           If a communication error is detected for the
           GPS function, a sensor, or other device, a
           warning will appear on the multi-function dis-
           play and the buzzer will sound. If this occurs,
           reduce the engine speed, return to shore, and
           have a Yamaha Boat Dealer check the boat.

           Low fuel level warning
           If “Fuel Level” appears on the multi-function
           display and the buzzer will sound, refill the

                                                                                 69

| 72 73 74 75 76 77 78 79 80 81 82 |