Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 201 - LIT-18626-12-95
P. 201

    Trouble recovery

                                                (4) Move the manual release levers of the
                                                   shift motors to the electronic operation
             1                                     position.

                                                Power steering system will not
                                                operate (252SD)
                                                If the power steering system malfunctions, a
                                                warning will appear on the multi-function dis-
                                                play and the direction of the boat cannot be
                                                changed even if the steering wheel is turned.
           1  Shift gate
           TIP:                                           S SEE  S S    S SW W
           z When the manual release levers are in the
                                                         Check Engine !
            manual operation position, the shift gates
                                                         Stop steering.
                                                         Open service valve of pump. Move cylinder to center  NEXT
            cannot be moved to the neutral or reverse  0 rpmpm  position. Using the two remote control levers, perform the boat  x x1000 1000
                                                  r
                                                 0
                                                         steering operation by the engine speed difference.
                                                         Consult YAMAHA dealer.  QUIT
            positions.
           z When the manual release levers are in the
            manual operation  position, the boat  will
                                                 Bilgee  Bl owe            Nav  Anchor r
                                                                                  o
                                                                                 h
                                                 B
                                                                           N
                                                                           av
                                                  lg
                                                      Blowerr
                                                  i
                                                                               A
                                                                                nc
            move forward even if the remote control le-
            vers are moved to the reverse position.
           z 252SD:  When the manual release levers  Manually point the jet thrust nozzles in the
            are in the manual operation position, the  straight-ahead direction, and then use  the
            boat will move forward even if the DRiVE  difference in the amount of throttle for the
            mode is activated  and the  throttle/shift  port and starboard engines to steer the boat
            paddle (left) is pulled.            and return to shore. After returning to shore,
           (7) Move  the manual release levers of  the  have a Yamaha Boat Dealer check the boat.
              shift motors to the electronic operation  TIP:
              position.                         If  a malfunction  is  detected for the power
           If the shift gates cannot be raised using the  steering system, the maximum engine speed
           preceding procedure, the shift gates can be  will be limited to approximately 5000 rpm.
           raised manually from the water.
           To raise the shift gates from the water:  To point the jet thrust nozzles in the straight-
           (1) Follow the above steps 1–4 for “To raise  ahead direction:
              the shift gates”.                 (1) Stop the engines  and remove the clip
           (2) Enter the water and move to the rear of  from the engine shut-off switch.
              the boat.                         (2) Open the driver’s side console compart-
           (3) Raise the shift gates to the forward posi-  ment. (See page 107.)
              tion.                             (3) Turn the  service valve on  the steering
                                                   pump in the direction shown in the illus-
                                                   tration.
                                                                                193

| 196 197 198 199 200 201 202 203 204 205 206 |