Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 132 - LIT-18626-12-95
P. 132

    Equipment operation

                       Bimini top               (3) Insert the front support poles into  the
                (AR250 / 252S / 252XE)             mounting holes in the wakeboard tower.
           Setting up the bimini top
           To set up the bimini top:                                    2
           (1) Remove the storage cover, and then un-
              wrap the bimini top.

                       1                          1

                                                1  Mounting hole
                                                2  Front support pole
                                                (4) Pull the rear of the bimini top toward the
                                                   stern, and then unhook the rear support
           1  Storage cover
                                                   poles from the main pole.
           (2) Pull the front of the bimini top toward the
              bow, and then open the flap and pull out
              the front support poles from the bimini
              top.                                                    2

                               1

                                                                1

                                                1  Rear support pole
                                                2  Main pole
                                  2

           1  Front support pole
           2  Flap

           124

| 127 128 129 130 131 132 133 134 135 136 137 |