Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-95
P. 50

    Control function operation

                                                  turn to the neutral position and the engines
             1                                    will return to idle speed.

                                                                      1

             2
                                                       2

           1  Shift gate
           2  Jet thrust nozzle
                                                1  Throttle/shift paddle (right)
           Throttle/shift paddles (252SD)       2  Throttle/shift paddle (left)
           When the DRiVE mode is activated, the throt-
           tle/shift paddles can be used at low speeds  TIP:
           to control the throttle and shifting instead of  z If the operator pulls both throttle/shift pad-
           the remote control levers. When making  dles until they stop, the reverse operation
           small throttle  adjustments for  docking, the  has priority.
           operator can use the throttle/shift paddles to  z When the DRiVE mode is activated, the en-
           operate the boat smoothly forward and in re-  gine speed for forward operation is limited
           verse while keeping both hands on the steer-  to approximately 3000 rpm and the engine
           ing wheel. (See page 79 for information on  speed for reverse operation is limited to ap-
           the DRiVE mode.)                       proximately 3500 rpm.
           z When the operator  pulls  the throttle/shift  z If either throttle/shift paddle is pulled while
            paddle (right), the shift gates for both en-  starting the  engines, the  engines will not
            gines will move to the TDE position, the en-  start.
            gine speed will increase, and the boat will
            move forward at a slow speed. When the  Reverse
            operator releases the throttle/shift paddle  The shift gates are dropped all the way down
            (right), the shift gates will return to the neu-  over the jet thrust nozzles. Jet thrust is redi-
            tral position and the engines will return to  rected  toward  the bow of the  boat, which
            idle speed.                         moves the boat backward.
           z When the operator  pulls  the throttle/shift
            paddle  (left), the shift  gates for  both en-
            gines will move to the reverse position, the
            engine speed will increase, and the boat
            will start moving in reverse at a slow speed.
            When the operator releases  the throt-
            tle/shift paddle (left), the shift gates will re-

           42

| 45 46 47 48 49 50 51 52 53 54 55 |