Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 200 - LIT-18626-12-95
P. 200

    Trouble recovery

           TIP:
           The rear platform hatch has interlocks to shut
           off the engines should the hatch be acciden-
           tally opened during operation.  The engines
           will not restart unless the hatch is closed and
           latched.

           Raising the shift gates
           (252SE / 252XE / 252SD)                1
           If the shift actuator malfunctions and the shift
           gates remain in the lowered position, the boat  1  Manual release lever
           will not be able to move forward.
           After raising the shift gates so that the boat  (5) Use a screwdriver or similar tool to re-
           can move forward, immediately return to  move the shift rod covers.
           shore and have a Yamaha Boat Dealer ser-
           vice the boat.                                    1
           To raise the shift gates:
           (1) Stop the engines and remove the clip
              from the engine shut-off switch.
           (2) Open the driver’s side console compart-
              ment. (See page 107.)
           (3) Remove the nuts, and then remove the
              shift motor cover.

                  1                             1  Shift rod cover

                                                (6) Slide the shift rods to port (left) to raise
                                                   the shift gates to the forward position.

                                          2

                                                                     1
           1  Shift motor cover
           2  Nut
           (4) Move  the manual release levers of  the
              shift motors to the manual operation po-
              sition.
                                                1  Shift rod

           192

| 195 196 197 198 199 200 201 202 203 204 205 |