Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 100 - LIT-18626-12-95
P. 100

    Instrument operation

           Language setting screen              er use  only, please  consult your  dealer if
           The language for the  multi-function  display  something was accidentally changed.
           unit can be changed.
                                                To drain the water in a ballast tank:
                                                (1) Touch and hold the setting screen tab for
                        Set Language
                                                   5 seconds.
                                                (2) Tap the “Ballast Times” button.
                    English     Espanol

                          Francais
                                                             Diagnostics Menu
                                                        Port Engine  Starboard Engine
              Back                                    PDM Diagnostics  Software Information
                                                          BCU       Ballast Times

           To change the language, tap the desired lan-
           guage.                                                          Load Software

           Tuner Region setting screen
           Set the region in which the multi-function dis-  (3) Tap the “Flush-Out Ballasts” button.
           play unit will be used.

                                                             Diagnostics Menu
                         Tuner Region
                                                              Ballast Times
                  North America  South America
                                                             Flush-Out Ballasts
                    Japan        Taiwan
                                                   Back
              Back

                                                (4) Tap the “OFF” button to change it to
           To change the tuner region, tap the desired  “ON” to start draining the water.
           region.

           Flush-out ballasts (252XE)
           The flush-out ballasts can be used to drain
           the water in the ballast tanks with the multi-
           function display unit.
           TIP:
           The diagnostics menu is for dealership use.
           All other functions on this screen are for deal-

           92

| 95 96 97 98 99 100 101 102 103 104 105 |