Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 113 - LIT-18626-12-95
P. 113

    Equipment operation

           (2) Turn the lock handle counterclockwise-  Rear underseat storage compartment
              and make  sure that  the lid is  securely  (starboard)
              closed.                            NOTICE
           (3) Push the lock handle down.
           To drain water from the ski locker:  252XE: This storage compartment con-
           (1) Remove the drain plug on the bottom of  tains a ballast tank. Be careful not to store
              the ski locker to drain the water.  items in this area that could be crushed or
                                                might damage the ballast tank.

                                                The rear underseat  storage compartment
                                                (starboard) is located  under  the rear star-
                                                board seat.
                                                To open the rear underseat storage compart-
                                                ment (starboard), lift the rear starboard seat
                                                up.
                               1

                                                                              1
           1  Drain plug

           (2) Securely install the drain plug in its origi-
              nal position.

                                                1  Rear starboard seat

                                                                   1

                                                1  Rear underseat storage compartment (star-
                                                   board)

                                                                                105

| 108 109 110 111 112 113 114 115 116 117 118 |