Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 202 - LIT-18626-12-95
P. 202

    Trouble recovery

                                 1

                                                       1          2

           1  Service valve                     1  Cable holder
                                                2  Edge of the bracket
           (4) Open the front underseat storage com-
              partment (starboard), and then open the  (6) Tighten the service valve.
              box to access the steering cylinder.
                                                To change the steering direction of the boat:
                                       1        Activate the running mode and use the differ-
                                                ence in the amount of throttle for the port and
                                                starboard engines.
                                                Turning to port

                                                                        F
                                                                        N
           1  Steering cylinder
                                                                        R
           (5) Move the cable holder manually  and
              align the end of the rod with the edge of
              the bracket.
                                                Turning to starboard

                                                                        F
                                                                        N
                                                                        R

           194

| 197 198 199 200 201 202 203 204 205 206 207 |