Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 83 - LIT-18626-12-95
P. 83

    Instrument operation

           z Push the “CRUISE/NO  WAKE” (–) button
            repeatedly until “No Wake” disappears.
           z Push the remote control levers forward to
            open the throttle.

           Operating the boat in reverse with
           more thrust (reverse RPM control)
           Engine speed in reverse is limited to approx-
           imately 4500 rpm. If more thrust is required
           when the boat is traveling in reverse, use the
           reverse RPM control.  WARNING! Be pre-
           pared to reduce throttle as soon  as the
           boat moves  as desired.  Otherwise, the
           boat may become unstable, which could
           result in loss of control and an accident.
           To activate the reverse RPM control:
           (1) Move the remote control levers back-
              ward so that the throttle is opened in re-
              verse and both engines are operating at
              the same engine speed.
           (2) Increase the engine speed to 4500 rpm,
              and then push the “CRUISE/NO WAKE”
              (+) button.
           Once the reverse RPM control is activated,
           pushing the “CRUISE/NO WAKE” (+) button
           will increase the available  engine speed by
           approximately 500 rpm in 3 stages up to a
           maximum  of 6000 rpm, and pushing  the
           “CRUISE/NO WAKE” (–) button will decrease
           the available engine speed. However, the ad-
           justment is limited to these 3 increments.
           To deactivate the reverse RPM control:
           Operate the remote control  levers  to de-
           crease the engine speed to less than 4500
           rpm.

                                                                                 75

| 78 79 80 81 82 83 84 85 86 87 88 |