Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 204 - LIT-18626-12-95
P. 204

    Trouble recovery

           Fuse replacement
                                                    1 23      4   5      6 7
               WARNING
           Do not use  fuses  of a higher amperage
           than recommended. Substitution with  a                              8
           fuse that has an improper rating can cause                          9
           extensive electrical system  damage  and
           possible fire.
                                                                               8
           If a fuse is blown, replace it with the proper
           fuse.                                            11      10
           To replace a fuse:                   1  Electronic throttle valve fuse
           (1) Open the engine hood. (See page 103.)  2  Fuel pump fuse
           (2) While pushing both sides of the fuse box  3  Main relay drive fuse
              cover inward, pull the cover toward the  4  Main fuse
                                                5  Spare fuse (252SE / 252XE / 252SD)
              bow and remove it.
                                                6  Fuse puller
                                                7  Battery fuse (AR250 / SX250 / 252S)
                                                8  Screw (252SE / 252XE / 252SD)
                                                9  BCU fuse (252SE / 252XE / 252SD)
                                                10 Spare fuse
                           1                    11 Unused fuse

                                                (3) 252SE / 252XE / 252SD: When replacing
                                                   the BCU fuse, remove the screws, and
                                                   then remove the fuse. Install the spare
                                                   fuse, and then tighten the screws.
                                                (4) When replacing an accessory fuse,  re-
           1  Fuse box cover
                                                   move the accessory fuse holder or cov-
                                                   er. (Open the rear underseat storage
                                                   compartment [port] to access the acces-
                                                   sory fuse. [See page 106.])

           196

| 199 200 201 202 203 204 205 206 207 208 209 |