Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 117 - LIT-18626-12-95
P. 117

    Equipment operation

                                           2

                                                                              2
                                                  1

                                      1
                                                  3

           1  Glove compartment lid             1  Galley storage compartment lid
           2  Glove compartment latch           2  Galley storage compartment lid latch
                                                3  Cooler box

                                                To close the galley storage compartment:
                                                Close the galley storage compartment lid,
                                                and then push it to securely lock it in place.
                                       1
                                                To extend the galley table:
                                                (1) Open the cushion at the rear of the gal-
                                                   ley, and lift up the galley table.

           1  Glove compartment

           To close the glove compartment:
           Close the glove compartment lid, and  then
           push it to securely lock it in place.          1

           Galley storage compartment (252S /
           252SE / 252XE / 252SD)
           The galley storage compartment is located to  1  Galley table
           the rearward of the driver’s seat.
           There are a cooler box under the galley stor-  (2) Align the edge of the cushion with the
           age compartment.                        groove on the galley table.
           To open the galley storage compartment:
           Pull the galley storage compartment lid latch
           to open the lid.

                                                                                109

| 112 113 114 115 116 117 118 119 120 121 122 |