Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 168 - LIT-18626-12-95
P. 168

    Operation

              are stopped, the  boat will  go  straight  Boating with passengers
              even though the steering wheel is turned.
                                                    WARNING
              You need throttle to steer.
                                                When  passengers are on board,  make
           D                                    sure they are seated and holding onto the
                                                handgrips, handrails, or straps before you
                                                start  to accelerate. An  unprepared pas-
                                                senger could lose balance and fall.
                                                Your boat is designed for one operator and
                                                up to 11 passengers only. Never have more
                                                than 12 people in the boat. Passengers must
                                                sit in one of the seats and hold onto the hand-
                                                grips. Passengers should sit so the weight in
                                                the boat is balanced from side-to-side and
           Turning left                         bow-to-stern as much as possible. If the pas-
                                                senger seat in front of the helm is used, be
                                                sure  the operator’s  view ahead is not ob-
                                                structed.
                                                  Maximum load (252XE):
                                                    Total weight of cargo, operator, and
                                                    passengers:
                                                      1066 kg (2350 lb)
                                                    Total weight of operator and passen-
                                                    gers:
                                                      998 kg (2200 lb)
           Turning right
                                                  Maximum load (except for 252XE):
                                                    Total weight of cargo, operator, and
                                                    passengers:
                                                      1180 kg (2600 lb)
                                                    Total weight of operator and passen-
                                                    gers:
                                                      998 kg (2200 lb)

           160

| 163 164 165 166 167 168 169 170 171 172 173 |