Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 110 - LIT-18626-12-95
P. 110

    Equipment operation

                                                To install an underwater seat, fit the seat pole
                          1                     into the  seat  bracket,  and then secure the
                                                pole by inserting the lock pin.

                                                                            2

           1  Swim platform seat
                                                      1        3
           Underwater seats
           The underwater seats can be used to sit in  1  Seat bracket
           the water  while  the boat is  moored or an-  2  Seat pole
           chored.                              3  Lock pin
           Remove the seats  before starting the en-
           gines,  and install  the seats only  when the  TIP:
           boat is stopped and the engines are not run-  z The underwater seats can also be installed
           ning.                                  upside down to use as beverage holders.
                                                z The underwater seats will float if acciden-
               WARNING
                                                  tally dropped into the water.
           Do not sit on the underwater seats while
           the engines  are running.  Exhaust gases
           coming from underneath the swim plat-
           form contain carbon monoxide, a color-
           less, odorless gas which may cause brain
           damage or death when inhaled.

                                1

           1  Underwater seat

           102

| 105 106 107 108 109 110 111 112 113 114 115 |