Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 147 - LIT-18626-12-95
P. 147

    Operation and handling requirements

           Draining the bilge water on water
           This model is equipped with a self-draining
           deck and bilge pump to drain the bilge water
           on water.

           Self-draining deck
           Most water that enters the deck area drains
           automatically out the stern through the large
           drain hole in the deck.                                              1
           A one-way check valve in the drain prevents
           water from traveling back to the deck while
                                                1  Bilge pump outlet
           the boat is moored or moving in reverse.
                                                TIP:
           Bilge pump                           z 252S / 252SE / 252SD: The “BILGE” switch
           Your boat is equipped with a drainage sys-
                                                  light comes on while the bilge pump is op-
           tem that channels water that enters the boat
                                                  erating.
           from the storage compartments to the bilge
                                                252S
           under the engine compartment.
           When the “Bilge” button is tapped, the bilge
           pump will operate.
                                                                           1
                      NW    N     NE
             FUEL                        DEPTH
             50  %       FLOAT MODE       0  Ft
                                °F
                         Water Temp
               START                    HOUSE
               36.3  V                  11.8  V
               Bilge  Blower        Nav  Anchor  1  “BILGE” switch
               1                                252SE / 252SD
           1  “Bilge” button

                                                                           1

                                                1  “BILGE” switch

                                                                                139

| 142 143 144 145 146 147 148 149 150 151 152 |