Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-12-95
P. 93

    Instrument operation

                 Drive control screen           TIP:
           This screen can be used to set a target speed  z If the remote control levers are  moved
           for the boat, increase the set speed.  slowly to the fully open position, the boat
                                                  may not accelerate according to the select-
                WKS  WKB                          ed acceleration profile or reach the set tar-
                Target Speed   21.0               get speed.
                                                z If the single lever mode is activated, move
                Acceleration   Fast
                                                  only the remote control lever for the port
                                                  engine to the fully open position. (See page
                                                  79 for information on the single lever mode
                                                  button.)
                                                z 252SD: While the DRiVE mode is activated,
               Set                      Save
                                                  the drive control mode cannot be used.
                                                To deactivate the drive control:
           To activate the drive control:
                                                (1) Return the remote control levers to the
           (1) Tap the tab you want to set.
                                                   neutral position.
           (2) Tap the target speed.
                                                (2) Tap the “CANCEL” button.
           (3) To set  the speed,  tap each digit and
              scroll up or down, and  then tap the
              “Back” button.

                       8         0

                       9         1

           (4) Tap the desired acceleration profile.
           (5) Tap the “Set” button, and then tap the
              “Save” button.
           (6) Select the characters  you want to  set,
              tap the “Save” button.
           (7) After setting the preceding items, tap the
              “Set” button.
           (8) Move the remote control levers to the ful-
              ly open position.

                                                                                 85

| 88 89 90 91 92 93 94 95 96 97 98 |