Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-12-95
P. 80

    Instrument operation

              Multi-function display unit       Volume control mode
                       operation                Turn the joystick knob to change the audio
                                                volume.
           Because the multi-function display unit is
           equipped with a touch screen, you can touch
           the display directly to operate  the display
           functions.                                            VOLUME
                                                                 (SCROLL)
           In addition to touching the display, you can      HOME   CANCEL
           use the joystick to operate the display func-
           tions.                                                        1

           Touching the multi-function display                 CRUISE  CRUISE
                                                                   NO WAKE
                                                               NO WAKE
                                                1  Joystick knob
                                   RUNNING MODE
                         SE  S  SW
               FUEL                     DEPTH
               100 %                    .8 9  ft  Navigation control mode
                 19                   19
                    x1000 rpm     x1000 rpm     (1) Turn the joystick knob to change the se-
                           MPH
                 START                HOUSE        lected setting or item.
                13.0  V  9          9  13.0  V
                     Bilge  Blower  Nav  Anchor
                                                                 VOLUME
                                                                 (SCROLL)
                                                             HOME   CANCEL
           Using the joystick                                            1
           This joystick has the following two operation
           modes.
                                                               CRUISE  CRUISE
           z Volume control mode
                                                               NO WAKE
                                                                   NO WAKE
           z Navigation control mode
           Push the  “VOLUME–(SCROLL)” button to
                                                1  Joystick knob
           switch the operation mode.
                            1                   (2) Push the joystick knob to select an item
                                                   or confirm a setting.
                           VOLUME
                           (SCROLL)
                        HOME   CANCEL

                         CRUISE  CRUISE
                         NO WAKE  NO WAKE

           1  “VOLUME–(SCROLL)” button

           72

| 75 76 77 78 79 80 81 82 83 84 85 |