Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-95
P. 48

    Control function operation

                                                ward position,  and then as the  levers are
                                                moved farther, accelerates  the  engines for
                                                more thrust. Moving the levers back from the
                                                neutral position shifts into the reverse posi-
                                                tion, and then as the levers are moved farther,
                                                accelerates the engines for more thrust.
                                                AR250 / SX250 / 252S: For cruising, adjust
                                                the remote control levers so both engines are
                                                running at the same engine speed.
                            1                   TIP:

           1  “START/STOP” button               Because of the mechanical throttle linkage,
                                                the remote control levers may not be exactly
           TIP:                                 even with one another when the engines are
           z The engine will not start when the clip is re-  running at the same engine speed.
            moved from the engine shut-off switch.
           z The main switch will not operate (the starter
                                                                 N
            motor  will not turn over) if the “START”    2       1
                                                       F     5        5    R
            switch in the rear underseat storage com-   3                 4
            partment (port) is turned to the OFF posi-
            tion. (See page 37 for more information.)  7                      7
                                                               6     6
           Remote control levers                 8                               8
               WARNING
           z Before shifting, make sure there are no
            swimmers  or obstacles in the water
                                                1  Neutral position
            near you.                           2  TDE position
           z When operating in reverse, go slowly.  3  Forward position
            Do not open the throttle more than half.  4  Reverse position
            Otherwise, the boat may become unsta-  5  Shift
            ble, which could result in loss of control  6  Fully closed
            and an accident.                    7  Throttle
           z Do not shift into reverse while traveling  8  Fully open
            at planing speeds. Loss of control, boat
                                                TIP:
            swamping, or damage to the boat could
                                                This boat is equipped with a “start-in-gear”
            occur.
                                                protection. The engines will not start unless
           The remote control lever for each engine con-  the levers are in the neutral position.
           trols both throttle and shifting. In normal op-
           eration, the levers are moved together.  This boat uses a direct-drive propulsion sys-
           Moving the  remote control levers  forward  tem. Therefore, jet thrust is always being pro-
           from the neutral position shifts into the for-  duced while the engines  are  running. The

           40

| 43 44 45 46 47 48 49 50 51 52 53 |