Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 23 - LIT-18626-12-95
P. 23

    Safety information

              Operational requirements          z Attach the engine shut-off cord (lanyard) to
           z The operator and all passengers must wear  the PFD and keep it free from the steering
            a U.S. Coast Guard (USCG) approved per-  wheel or other controls so that the engines
            sonal flotation device (PFD).         stop if the operator accidentally leaves the
                                                  helm. Failure to attach the engine shut-off
                                   1              cord (lanyard) could  result in a runaway
                                                  boat if the operator is ejected.
                                                  After operation, remove the engine shut-off
                                                  cord (lanyard) and the main switch keys to
                                                  avoid accidental starting or unauthorized
                                                  use by children or others.

                                                AR250 / SX250 / 252S

           1  PFD                                            1
           z Eye protection is recommended to keep
            wind, water, and glare from the sun out of                2
            your eyes while you operate your boat. Re-
            straining straps for eyewear are made
            which are designed to  float should  your
            eyewear fall in the water.
           z Never operate the boat after consuming al-
            cohol or taking drugs.              1  Engine shut-off switch
                                                2  Engine shut-off cord (lanyard)
           z For reasons of safety and proper care of
            the boat, always perform the pre-operation
                                                252SE / 252XE / 252SD
            checks listed on page 142 before operating
            the boat.
           z Passengers must always sit in a designat-
            ed seating area, place  feet  on the deck,                 2
            and hold on to the handgrips, handrails, or
            straps when the boat is in motion.
           z Always consult your doctor on whether it is   1
            safe for you to ride in this boat if you are
            pregnant or in poor health.
           z Do not attempt to modify this boat.
            Modifications  to  your boat may reduce
                                                1  Engine shut-off switch
            safety and reliability, and render the boat
                                                2  Engine shut-off cord (lanyard)
            unsafe or illegal to use.

                                                                                 15

| 18 19 20 21 22 23 24 25 26 27 28 |