Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-12-95
P. 82

    Instrument operation

           running above  3000  rpm and below  7000  When “Cruise” and the cruise assist setting
           rpm.                                 level disappear, the cruise assist is deactivat-
           To activate the cruise assist:       ed.
           (1) Push the remote control levers forward
              to open the throttle until the desired en-  Operating the boat with a minimal
              gine speed is reached and both engines  wake (no-wake mode)
              are operating at the same engine speed.  The no-wake mode is useful for operating the
           (2) Push the “CRUISE/NO WAKE” (+) button  boat at a steady speed with a minimal wake.
              or “CRUISE/NO WAKE” (–) button. When  This is especially convenient when traveling
              the cruise assist is activated, “Cruise”  in harbors, channels, or other areas posted
              and the cruise assist setting level will be  with low speed limits as “no wake zones”.
              displayed under the boat speed.   The no-wake mode can be  activated only
                                                when the engines are operating at idle speed.
                    SE      S      SW           To activate the no-wake mode:
                                                (1) Put the remote control levers in the TDE
                                                   position or forward position so that both
                                                   engines are operating at idle speed.
                                                (2) Push the  “CRUISE/NO WAKE” (+) but-
                           MPH                     ton. When the no-wake mode is activat-
                                                   ed, “No Wake” will be displayed under
                          Cruise +4
                                                   the boat speed.
                              1
                                                          SE     S      SW
           1  Cruise assist setting level
           z Once the cruise assist is activated, the set
            engine speed can be increased by pushing
            the “CRUISE/NO WAKE” (+) button or de-
            creased by  pushing the  “CRUISE/NO                 MPH
            WAKE” (–) button. However, the  adjust-            No Wake
            ment is limited to a maximum of 8 incre-
            ments above or below the initial cruise              1
            assist setting. Each  time a button is  1  “No Wake”
            pushed, the engine speed will increase or
            decrease approximately 100–200 rpm.  The no-wake mode can be set to 3 engine
           z While the cruise assist is activated, the en-  speeds. To adjust the engine speed while the
            gine speed can also be adjusted by operat-  no-wake  mode is activated, push the
            ing the remote control levers.      “CRUISE/NO   WAKE”   (+)  button  or
                                                “CRUISE/NO WAKE” (–) button.
           To deactivate the cruise assist:     To deactivate the no-wake mode:
           Operate the remote control  levers  to de-  Perform one of the following operations.
           crease the engine speed to 3000 rpm or less.

           74

| 77 78 79 80 81 82 83 84 85 86 87 |