Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 145 - LIT-18626-12-95
P. 145

    Operation and handling requirements

           4-star models                        4-star models

                             1
                                                                         1
                                                                           2

           1  Dipstick                          1  Maximum level mark
                                                2  Minimum level mark
           (4) Insert the dipstick back into the dipstick
              tube  completely. Remove the  dipstick  (5) If the engine oil  level  is  significantly
              again and check that the engine oil level  above the maximum level mark, consult
              is between the minimum level mark and  a Yamaha Boat Dealer. If the engine oil
              maximum level mark.                  level is below the minimum level mark,
           3-star models                           add engine oil.
                                                (6) Remove the engine oil filler cap.

                                  1                                      1
                                     2

           1  Maximum level mark
           2  Minimum level mark
                                                1  Engine oil filler cap
                                                (7) Slowly add engine oil.
                                                (8) Wait approximately 5 minutes to allow
                                                   the engine oil to settle, and then check
                                                   the engine oil level again.
                                                (9) Repeat steps 3–8 until the engine oil is at
                                                   the proper level.
                                                (10) Install the engine oil filler cap.
                                                (11) Repeat the checking oil level procedure
                                                   for the other engine.
                                                (12) Close the engine hood.

                                                                                137

| 140 141 142 143 144 145 146 147 148 149 150 |