Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 87 - LIT-18626-12-95
P. 87

    Instrument operation

           Operation mode                       DRiVE mode “  ” (252SD)
           When the engines are running and both re-  Both engines are operated at the same en-
           mote control levers are in the neutral position,  gine speed and  the throttle  and shifting of
           the operation mode can be changed by tap-  both engines are controlled using the left and
           ping the operation mode button.      right throttle/shift paddles. “DRiVE” is shown
                                                for the mode status.
                            1     2
                                                Use this mode to make small throttle adjust-
                                                ments  when operating  the boat at  slow
                          RUNNING MODE
                                                speeds, such as when docking. (See page 42
                 SW
                 NE
                                    DEPTH       for information on the throttle/shift paddles.)
                                    .8 9  ft
                                  19
                         x1000 rpm              TIP:
                                                z If the remote control levers are moved from
            H
                                 HOUSE            the neutral position to the forward or re-
                             9   13.0  V
                   Nav  Anchor                    verse position while the throttle/shift pad-
                                                  dles are not being operated, the operation
           1  Mode status
           2  Operation mode button               mode will change to the running mode.
                                                z When the DRiVE mode is activated, the en-
           Float mode                             gine speed will be controlled.
           Both engines are stopped. “FLOAT-MODE”
           is shown for the mode status.
           The audio system function and water temper-
           ature are shown instead of the port and star-
           board tachometers.

           Running mode “  ”
           The port and starboard remote control levers
           control the throttle and shifting for their re-
           spective engines.  “RUNNING-MODE” is
           shown for the mode status.

           Single lever mode “  ”
           Both engines are operated at the same en-
           gine  speed and the throttle  and shifting of
           both  engines are  controlled using only  the
           port remote control lever. “SINGLE-LEVER”
           is shown for the mode status.
           The starboard remote control lever is not
           used.

                                                                                 79

| 82 83 84 85 86 87 88 89 90 91 92 |