Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 187 - LIT-18626-12-95
P. 187

    Maintenance

                     Maintenance                Removing and installing the engine
                                                covers
               WARNING
                                                The engine cover of each engine is remov-
           Be sure to turn off the engines when you  able.
           perform maintenance  unless otherwise  To remove the engine cover:
           specified. If you are not familiar with ma-  (1) Open the engine hood. (See page 103.)
           chine servicing, this work should be done  (2) Remove the engine cover screws.
           by a Yamaha Boat Dealer or other quali-
           fied mechanic.
           Maintenance, replacement, or repair of  the
           emission control devices and system may be                        1
           performed by any marine SI engine repair es-
           tablishment or individual. Warranty repair,
           however, must be performed at an autho-
           rized Yamaha Boat Dealer. A service manual
           is available for purchase through a Yamaha
           Boat Dealer for owners  who have the me-
           chanical skills, tools, and other equipment  1  Engine cover screw
           necessary to perform maintenance not cov-
                                                (3) Lift up the engine cover and remove it.
           ered by this owner’s/operator’s manual.
           Owner’s/operator’s manual
           It is advisable to always carry the own-
           er’s/operator’s manual with  you whenever                       1
           you use the boat.
           To protect these materials from water dam-
           age, it would be a good idea to put them in a
           waterproof bag. If  your owner’s/operator’s
           manual is damaged, order a replacement
           from a Yamaha Boat Dealer.
           The service information included in this man-  1  Engine cover
           ual is intended to provide you, the owner,
           with the necessary information for complet-  To install the engine cover:
           ing  your own preventive  maintenance and  (1) Place the engine cover in its original po-
           minor repairs.                          sition, and then push it down.

                                                                                179

| 182 183 184 185 186 187 188 189 190 191 192 |