Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 157 - LIT-18626-12-95
P. 157

    Pre-operation checks

           Blower checks
               WARNING                                      NW    N    NE
                                                   FUEL                        DEPTH
           Gasoline vapors can explode.  Before   50  %       FLOAT MODE       0  Ft
           starting the engines, check the engine
                                                                     °F
           compartment for gasoline, gasoline va-
                                                               Water Temp
           pors, and loose electrical connections,
                                                     START                   HOUSE
           and then operate the blowers for at least 4  36.3  V              11.8  V
           minutes. Do not start the engines or oper-  Bilge  Blower     Nav  Anchor
           ate the blowers if you can smell gasoline     1
           vapors in the  engine compartment or if
                                                1  “Blower” button
           there are any loose electrical connections.
           Contact a Yamaha Boat Dealer if there is a
                                                252S / 252SE / 252SD
           problem you cannot locate or correct.
                                                To check the operation using the switch pan-
           Make sure that the blowers operate properly.  el:
                                                Push the “BLOWER” switch. Check that the
                                     1          blowers operate when the switch light is on
                                                and that the blowers stop when the switch
                                                light is off.
                                                252S
            1

                                                                            1

           1  Blower
           To check the operation using the multi-func-
           tion display:
           Tap  the “Blower” button.  Check that the
                                                1  “BLOWER” switch
           blowers operate when the button is blue and
           that the blowers stop when the button is gray.

                                                                                149

| 152 153 154 155 156 157 158 159 160 161 162 |